|  |  |  |
| --- | --- | --- |
| **INNOVTECH M1850 18.5 Inch E-LED Display** | | |
| **PANEL** | Screen Size | 18.5" |
| Display Type | E-LED |
| Resolution | 1366x768 |
| Aspect Ratio | 16:9 |
| Brightness | 210cd/m2 |
| Static Contrast Ratio | 1000:1 |
| Refresh Rate | 60Hz |
| Viewing Angle (H/V) | 170°/160°TN |
| Response Time | 5ms (OD) |
| Color | 16.7M |
| Life Time | Life Time |
|  |  |
| **STRUCTURAL** | Front Bezel | Plastic |
| Rear Cover | Plastic |
| Stand | Plastic |
| Base | Plastic |
| Tilt {Center to Front/Back} | -5°/15° |
| Free sync | YES |
| HDCP | 2.2 |
| Wall Mount | YES |
| **INTERFACE** | VGA | YES |
| DC IN | 1 |
| **FEATURES** | Main Board | RDT25UT |
| Key Board | 5 keys (Lever Type) |
| Boot Logo | Option |
| Color Temperature | WARM, COOL, User Mode |
| OSD Language | Multi Language |
| **POWER** | Input | 100~240VAC, 50/60Hz |
| Power Consumption | <40W |
| Max Stand by Power | <0.5W |
| Certification | FCC |
| Energy Efficiency Grade | DOE Level VI |
| **ENVIRONMENT CONDITION** | Operating Temperature | 0°C~40°C |
| Storage Temperature | -10°C~60°C |
| Operating Relative Humidity | ≤80% |
| Storage Relative Humidity | ≤80% |
| **VIDEO MODE** | SVGA（800x600) | YES |
| XGA（1024x768) | YES |
| WXGA (1280x600) | YES |
| WXGA (1280x720) | YES |
| WXGA (1280x768) | YES |
| WXGA（1360x768) | YES |
| WXGA（1366x768) | YES |
| **ATTACH** | AC Adapter | YES |
| Base | YES |
| User Manual | YES |
| VGA Signal Cable | YES |
| **DIMENSIONS (L X W X H)** | Packing Dimension | 490\*110\*352mm |
| Net Weight (With the Base) | 3.2kg |
| Gross Weight | 4.5kg |