|  |  |
| --- | --- |
| **Image Sensor** | CIS |
| **Light Source** | LED |
| **Optical Resolution** | 1200 dpi |
| **Hardware Resolution** | 1200 x 1200 dpi |
| **Scan Modes** | Color: 48-bit input, 24-bit output Grayscale: 16-bit input, 8-bit output B/W: 1-bit output |
| **Scanning Speed** | 5.5 sec (Color Mode, 300 dpi, A6) |
| **Scanning Area (W x L)** | Maximum: 104.9 x 500 mm (4.13" x 19.69") Minimum: 33 x 43 mm (1.3" x 1.7") TWAIN support 104.9 x 500 mm (4.13” x 19.69”) |
| **Acceptable Paper Weight (Thickness)** | Paper: 50 g/㎡ to 120 g/㎡ Plastic card: Non-Embossed up to 0.76 mm |
| **Daily Duty Scan ( Sheets )** | 800 |
| **Action Button** | Scan, Custom |
| **Power Supply** | USB Power: 5V / 0.5A |
| **Interface** | USB 2.0 |
| **Net Weight** | 0.19 Kgs (0.42 Lbs) |
| **Dimensions (W x D x H)** | 174.5 x 60.5 x 38.5 mm (6.87" x 2.38” x 1.52”) |
| **Protocol** | TWAIN Compliant |
| **OS** | Windows 7 / 8 / 10 / 11 Linux compatibility is only available for system integrators. Please contact sales@plustek.com for more info. |
| **Hardware Requirements** | 2.0 GHz CPU processor or higher[1] [1]Windows Recommended: 2.8 GHz Intel® Core™ i5 Processor with 4 CPU Cores or higher 4 GB RAM minimum (Recommended: 8 GB or more) 6 GB of hard-disk space for program installation BUS Powered Display dimensions of 1024x768 or greater |
| **Bundled Software** | Plustek DocAction Plustek DocTWAIN ABBYY FineReader 12 Sprint NewSoft Presto! BizCard 6 |