|  |  |  |  |
| --- | --- | --- | --- |
| Product | **Requirements** | **AVR 1000VA** | |
| **Power (VA)** |
| Input | Phase | Single phase | |
| Voltage(1) | AC 110V-250V | |
| Voltage(2) | AC 100V-250V | |
| Frequency | 50Hz/60Hz | |
| Output | Voltage | AC220V/110V | |
| Precision | ±3% | |
| Capacity | 1000W | |
| Frequency(Inverter Mode) | 50Hz/60Hz | |
| Power Factor | 100%when input voltage 220V | |
| Function | Control Type | relay | |
| Over/Low Volt Protection | yes | |
| Delaying | yes | |
| Temperature Protection | temperature protection option | |
| Short Circuit & Over Load | Fuse protection | MCB |
| Efficiency | Ac-Ac | 0.96 | |
| Acoustic | Noise Level | <<50db | |
| Environmental | Temperature | -5-60 Degree | |
| Humidity | 20% to90% | |

**SAKO Single Phase -1000 VA Relay type**