|  |
| --- |
| **VA2256-H 22" 1080p Home and Office Monitor** |
| **DISPLAY** | Monitor Size: 22”W (21.5” Viewable) LCD monitor |
| Panel Technology: IPS Technology |
| Resolution: Full HD 1920 x 1080 |
| Display Area: 476.1mm (H) x 267.8mm (V) |
| Aspect Ratio: 16:9 |
| Brightness: 250 cd/m² (Typ) |
| Contrast Ratio: 1000:1 (Typ) |
| Dynamic Contrast Ratio: 50,000,000:1 |
| Viewing Angles: 178 degrees / 178 degrees (Typ) |
| Response Time: GTG: 5ms (Typ) |
| Refresh Rate (Hz): 75 |
| Response Time: GTG: 5ms (Typ) |
| **INPUT SIGNAL** | **Frequency:**24 ~ 83KHz ; Fv = 50 ~ 75Hz, |
| Sync: Separate Sync, TMDS |
| **COMPATIBILITY** | PC: Windows 7, Windows 8, Windows 8.1, Windows 10 certified |
| Mac®: mac OS tested |
| **CONNECTOR** | Input: VGA x 1, HDMI x 1 (v1.4 compatible) |
| Output: Earphone out x 1 (3.5mm plug) |
| **POWER** | Power: 3-pin Socket (IEC C14 / CEE22) |
| Voltage: AC 100-240V (Universal); 50/60Hz |
| Consumption: 25W |
| Optimize: 21W |
| Conserve: 18W |
| **ERGONOMICS** | Tilt: 20 ~ -4 degrees |
| **WALL MOUNT** | VESA®: 100 mm x 100 mm |
| **OPERATING CONDITIONS** | Temperature (º F / º C): 32°F to 104°F (0°C to 40°C)Humidity: 20% to 90% (no condensation) |
| **DIMENSIONS (W x H x D) (mm)** | Physical with stand (mm): 490mm (W) x 362mm (H) x 198mm (D) |
| Physical without stand (mm): 490mm (W) x 297mm (H) x 48mm (D) |
| Packaging (mm): 544mm (W) x 384mm (H) x 128mm (D) |
| **WEIGHT** | Net with stand: 3.3kg |
| Net without stand: 2.9kg |
| Gross: 4.8kg |
| **REGULATIONS** | cULus, FCC-B, ICES003, Energy Star 8.0, CEC, MX-CoC, Mexico Energy, RoHS, WEEE, VCCI, PSE, BIS, CCC, China RoHS, China Energy Label |
| **WARRANTY** | Warranty offered may differ from market to market |
| **PACKAGE CONTENTS** | LCD Display |
| 3-pin Plug (IEC C13 / CEE22) |
| HDMI Cable (Male-Male) x1 |
| Quick Start Guide |