|  |
| --- |
| **VA2405-H 24”1080p Monitor with HDMI and VGA Input** |
| **Display** | Display Size (in.): 24 |
| Viewable Area (in.): 23.6 |
| Panel Type: VA Technology |
| Resolution: 1920 x 1080 |
| Resolution Type: FHD |
| Static Contrast Ratio: 3,000:1 (typ) |
| Dynamic Contrast Ratio: 50M:1 |
| Light Source: LED |
| Brightness: 250 cd/m² (typ) |
| Colors: 16.7M |
| Color Space Support: 8 bit (6 bit + Hi-FRC) |
| Aspect Ratio: 16:9 |
| Response Time (Typical GTG): 4ms |
| Viewing Angles: 178º horizontal, 178º vertical |
| Backlight Life (Hours): 30000 Hrs (Min) |
| Curvature: Flat |
| Refresh Rate (Hz): 75Hz (Max)[1] |
| Adaptive Sync: Yes |
| Blue Light Filter: Yes |
| Flicker-Free: Yes |
| Color Gamut: NTSC: 72% size (Typ), sRGB: 104% size (Typ) |
| Pixel Size: 0.272 mm (H) x 0.272 mm (V) |
| Surface Treatment: Anti-Glare, Hard Coating (3H) |
| **Compatibility** | PC Resolution (max): 1920x1080 |
| Mac® Resolution (max): 1920x1080 |
| PC Operating System: Windows 10 certified; macOS tested |
| Mac® Resolution (min): 1920x1080 |
| **Connector** | VGA: 1 |
| HDMI 1.4: 1 |
| Power in: 3-pin Mickey Mouse Socket (IEC C6) |
| **Power** | Eco Mode (Conserve): 14W |
| Eco Mode (optimized): 17W |
| Consumption (typical): 20W |
| Consumption (max): 21W |
| Voltage: AC 100-240V, 50/60 Hz |
| Stand-by: 0.3W |
| **Additional Hardware** | Kensington Lock Slot: 1 |
| **Controls** | Physical Controls: Key 1 (favorite), Key 2, Key 3, Key 4, Key 5 (power) |
| On Screen Display: Input Select, View Mode, Color Adjust, Manual Image Adjust, Setup Menu |
| **Operating Conditions** | Temperature: 32°F to 104°F (0°C to 40°C) |
| Humidity (non-condensing): 20% to 90% |
| **Wall Mount** | VESA Compatible: 100 x 100 mm |
| **Input Signal** | Frequency Horizontal: 24 ~ 86KHz |
| Frequency Vertical: 48 ~ 75Hz |
| **Video Input** | Digital Sync: TMDS - HDMI (v1.4) |
| Analog Sync: Separate - RGB Analog |
| **Ergonomics** | Tilt (Forward/Back): -3º / 20º |
| **Weight (imperial)** | Net (lbs): 7.1 |
| Net Without Stand (lbs): 6.2 |
| Gross (lbs): 9.9 |
| **Weight (metric)** | Net (kg): 3.2 |
| Net Without Stand (kg): 2.8 |
| Gross (kg): 4.5 |
| **Dimensions (imperial) (wxhxd)** | Packaging (in.): 24 x 15.7 x 5.5 |
| Physical (in.): 21.6 x 16 x 7 |
| Physical Without Stand (in.): 21.6 x 12.8 x 1.6 |
| **Dimensions (metric) (wxhxd)** | Packaging (mm): 610 x 400 x 140 |
| Physical (mm): 548 x 406 x 177 |
| Physical Without Stand (mm): 548 x 324 x 41 |
| **General** | Regulations: cTUVus, FCC-B, ICES003, CEC, TUV S-Mark, MX-CoC, Mexico Energy, CE, CE EMC, CB, RoHS, ErP, REACH, WEEE, EAC, UkrSEPRO, UKCA, BSMI, RCM, GEMS, BIS, CCC, China RoHS, China Energy Label |
| PACKAGE CONTENTS: VA2405-H x1, 3-pin Mickey Mouse Plug (IEC C5) x1, HDMI Cable (Male-Male) x1, Quick Start Guide x1 |
| Recycle/Disposal: Please dispose of in accordance with local, state or federal laws. |
| Warranty: \*Warranty offered may differ from market to market |