|  |  |
| --- | --- |
| **VA708a 17" 5:4 Home and Office Monitor** | |
| **Display** | Type: TN  Display Area: 17" (5:4)  Resolution: 1280x1024 (SXGA)  Brightness: 250 cd/m² (Typ.)  Contrast Ratio: 1000 :1 (Typ.)  Viewing Angle: 170 (H) / 160 (V)  Response Time: Tr+Tf: 5ms (Typ.)  Refresh Rate (Hz): 75 (Max)[1]  Backlight Life: 30000 Hrs (Min.)  Colours: 16.7 M  Response Time: Tr+Tf: 5ms (Typ.) |
| **Compatibility** | PC: 1280x1024 |
| Mac®: 1280x1024 |
| **Connector** | Digital: VGA x1 |
| Power: Internal Power Board |
| **Power** | Voltage: AC 100-240V (Universal); 50/60 Hz |
| Consumption: 14W (Tpy.) |
| **Input Signal** | Frequency: 24 ~82 kHz / 50 ~75 Hz |
| Sync: Separate Sync |
| **ERGONOMICS** | Tilt: 20° ~ -3° |
| **OPERATING CONDITIONS** | Temperature: 32°F to 104°F (0°C to 40°C) |
| Humidity: 10% to 90% (no condensation) |
| **DIMENSIONS (L x H x P)** | Physical with stand: 366.9 (W) x 389.9 (H) x189.6 (D) mm |
| **WEIGHT** | Net with stand: 3.1kg |
| **PACKAGE CONTENTS** | LCD Display, Power Cable, Video Cable, Quick Start Guide |