|  |
| --- |
| **FLASH FL12A (ATX Gaming Case)** |
| **Feature** | **Eye-catching RGB LED Strip Design****Stylish Geometric Stripe Ventilation Area on Front Panel****USB Control Panel and Power Button on Top for User-friendly****Individual LED Button for Switching RGB Color****4 USB Ports and SD/TF Card Reader Available** |
| **Specification** | TYPE | ATX Case |
| DRIVE BAY : 5.25" | X |
| DRIVE BAY : 3.5" | 2 |
| DRIVE BAY : 2.5" | 2 |
| MOTHERBOARD | ATX / MICRO ATX |
| POWER SUPPLY | ATX PS/2, Bottom Mount |
| EXPANSION SLOT | 7 slots |
| STRUCTURE DIMENSION | 370x175x410mm |
| FAN CAPACITY : FRONT | 1x12cm |
| FAN CAPACITY : REAR | 1x8/9cm |
| FAN CAPACITY : TOP | X |
| MAX. CPU COOLER HEIGHT | 150mm |
| MAX. VGA CARD LENGTH | 340mm |