|  |  |  |
| --- | --- | --- |
| **MAR01A (ATX Gaming Case)** | | |
| **Feature** | **Transparent Tempered Glass Front Panel**  **Metal Mesh Strips Design on Two Sides for the Best Ventilation**  **Sleek Transparent Side Panel for Direct View of Inner System**  **USB Control Panel and Power Button on Top for User-friendly**  **Top / Bottom Anti-Dust Mesh Cover Included**  **Optional 3 \* 12cm LED Fans for Panel Decoration** | |
| **Specification** | TYPE | ATX Case |
| DRIVE SPACE : 3.5" | 2 |
| DRIVE SPACE : 2.5" | 2 |
| MAIN BOARD | ATX |
| POWER SUPPLY | PS2 |
| EXPANSION SLOT | 7 slots |
| STRUCTURE DIMENSION | 360x180x435mm |
| TYPE | ATX Case |
| DRIVE SPACE : 3.5" | 2 |
| CASE DIMENSION | 400x180x450mm |
| FAN CAPACITY FRONT | 3x12cm |
| REAR | 1x12cm |
| TOP | 2x12cm |
| MEASUREMENT | 1300PCS / 40'HQ |
| MAXIMUM  COMPATIBILITY  CPU Cooler: 150mm  M/B : 305x244mm | VGA Card Length: 320mm CPU Cooler: 150mm  M/B : 305x244mm |