|  |  |  |
| --- | --- | --- |
| **NEPTUNE NE07A (ATX Gaming Case)** | | |
| **Feature** | **Full Metal Mesh Front Panel Keep the Best Ventilation**  **Maximum Two 140mm Fans Behind the Mesh Front Panel**  **Control Panel with 4 USB Ports and Power Button on Top for User-friendly**  **Additional Exclusive LED Button for Switching RGB Fan Color Easily** | |
| **Specification** | TYPE | ATX Case |
| DRIVE SPACE : 5.25" | 0 |
| DRIVE SPACE : 3.5" | 2 |
| DRIVE SPACE : 2.5" | 2 |
| MAIN BOARD | E-ATX |
| POWER SUPPLY | PSII |
| EXPANSION SLOT | 7 slots + 2 (Vertical) |
| STRUCTURE DIMENSION | 380x210x440mm |
| FAN CAPACITY FRONT | 3x12cm or 2x19cm |
| FAN CAPACITY REAR | 1x12cm |
| FAN CAPACITY TOP | 2x12cm or 2x14cm |
| FAN CAPACITY BOTTOM | 2x12cm |
| SUPPORT VGA CARD LENGTH | 350mm |
| SUPPORT CPU COOLER | 160mm |