|  |
| --- |
| **RA08A(ATX Gaming Case)** |
| **Feature** | **Extremely Eye-catching with 3 LED Fans Installed in Front Panel****Sleek Transparent Side Panel for Direct View of Inner System****USB / Audio Ports on Top for User-friendly****Sufficient Cable Management Space for Easy System Installation and Expansion****Top / Bottom Anti-Dust Mesh Cover Included****Optional SD/TF Card Reader and Super Speed USB3.1 (Type-C)** |
| **Specification** | TYPE | ATX Case |
| DRIVE SPACE : 3.5" | 2 |
| DRIVE SPACE : 2.5" | 2 |
| MAIN BOARD | ATX |
| POWER SUPPLY | PS2 |
| EXPANSION SLOT | 7 slots |
| STRUCTURE DIMENSION | 360x205x430mm |
| CASE DIMENSION | 425x205x460mm |
| FAN CAPACITY FRONT | 3x12cm |
| REAR | 1x12cm |
| TOP | 2x12cm |
| MEASUREMENT | 1000PCS / 40'HQ |
| CASE DIMENSION | 425x205x460mm |
| FAN CAPACITY FRONT | 3x12cm |
| MAXIMUMCOMPATIBILITY | VGA Card Length : 325mmCPU Cooler : 160mmM/B : 305x244mm |