|  |  |  |
| --- | --- | --- |
| **F55A F-SERIES (ATX Gaming Case)** | | |
| **Feature** | **Simple and Noble Design**  **Aluminum Alike Surface Presents High Quality**  **Metal Mesh on Two Sides for the Best Ventilation**  **Top Control Panel with 3 \* USB + HD Audio for User-friendly**  **Super Speed USB3.0 is Ready for Option** | |
| **Specification** | TYPE | ATX Case |
| DRIVE SPACE : 5.25" | 1 |
| DRIVE SPACE : 3.5" | 2 |
| DRIVE SPACE : 2.5" | 2 |
| MAIN BOARD | ATX |
| POWER SUPPLY | PS2 |
| EXPANSION SLOT | 7 slots |
| STRUCTURE DIMENSION | 370x175x410mm |
| FAN CAPACITY FRONT | 1x12cm |
| FAN CAPACITY REAR | 1x8/9cm |
| FAN CAPACITY SIDE | 1x12cm |
| MEASUREMENT | 1420PCS / 40'HQ |
| SUPPORT VGA CARD LENGTH | 340mm |
| SUPPORT CPU COOLER | 145mm |
| SUPPORT M/B | 305x244mm |