|  |
| --- |
| **F88A F-SERIES (ATX Gaming Case)** |
| **Feature** | **Simple and neat design****Aluminum alike surface presents high quality****Piano-finished strips for decoration****Stylish Color Waved-shaped Bars****Top control panel with 4xUSB + HD audio for user-friendly****Super speed USB 3.0 is ready for option** |
| **Specification** | TYPE | ATX Case |
| DRIVE SPACE : 5.25" | 1 |
| DRIVE SPACE : 3.5" | 2 |
| DRIVE SPACE : 2.5" | 2 |
| MAIN BOARD | ATX |
| POWER SUPPLY | PS2 |
| EXPANSION SLOT | 7 slots |
| STRUCTURE DIMENSION | 370x175x410mm |
| CASE DIMENSION | 400x175x420mm |
| FAN CAPACITY FRONT | 1x12cm |
| FAN CAPACITY REAR | 1x8 or 9cm |
| FAN CAPACITY SIDE | 1x12cm |
| MEASUREMENT | 1420PCS / 40'HQ |
| SUPPORT VGA CARD LENGTH | 340mm |
| SUPPORT CPU COOLER | 145mm |
| SUPPORT M/B | 305x244mm |