|  |  |
| --- | --- |
| Native Resolution | 854x480 |
| Brightness | 120 (LED Lumens) |
| Contrast Ratio | 500:1 |
| Display Color | 1.07 Billion Colors |
| Light Source Type | LED |
| Light Source Life (hours) with Normal Mode | up to 30000 |
| Lamp Watt | RGB LED |
| Lens | F=1.7, f=7.5mm |
| Projection Offset | 0+/-5% |
| Throw Ratio | 1.2 |
| Optical Zoom | Fixed |
| Image Size | 24"-100" |
| Throw Distance | 0.64m-2.66m, (39" @1m) |
| Keystone | +/- 40° (V) |
| Audible Noise (Normal) | 26dB |
| Audible Noise (Eco) | 25dB |
| Local Storage | Total 8GB, (4GB available storage) |
| Input Lag | 35ms |
| Resolution Support | VGA (640 x 480) to FullHD (1920 x 1080) |
| HDTV Compatibility | 480i, 480p, 576i, 576p, 720p, 1080i, 1080p |
| Horizontal Frequency | 15h-102kHz |
| Vertical Scan Rate | 23-120Hz |
| **Input** | |
| HDMI | 1 |
| Audio-in (Bluetooth) | 1 (BT4.2) |
| USB Type A | 1, (USB2.0 Reader) |
| WIFI Input | 1 (5Gn) |
| **Output** | |
| Audio-out (Bluetooth) | 1 (BT4.2) |
| Speaker | 2W Cube |
| USB Type A (Power) | 1, (USB2.0 - 5V/1A, share with USB A Input) |